2020/08/24:

Switching from interior point methods to sqp, according to MATLAB this new method is faster.

It is not really working, switching to manual gradient descent.